;; Realtek RTLWLANE PCI-E Wireless LAN Network Interface Cards.
;;
;; Copyright 2012, Realtek Semiconductor Corporation
;;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%
CatalogFile = netrtwlane.cat                               ;; for WHQL certified
DriverVer = 04/19/2013,2007.12.0419.2013

[Manufacturer]
%Realtek% = Realtek,NTamd64.6.0
%Lenovo% = Lenovo,NTamd64.6.0
%ASUS% = ASUS,NTamd64.6.0
%Edimax% = Edimax,NTamd64.6.0

[ControlFlags]
ExcludeFromSelect = *

[Realtek.NTamd64.6.0]

;;*******************************************************************************
;; RTK COMMON DEVICE DESC
;;*******************************************************************************
;;----------------------------------------------------------------------------
;; For 8192C RTK common
;;----------------------------------------------------------------------------
%RTL8192ceT.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8191
%RTL8192ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_817810EC
%RTL8192ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_818610EC
%RTL8192ce.DeviceDesc%		= INTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_818310EC
%RTL8192ce.DeviceDesc%		= INTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_819110EC
%RTL8192ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_11781A3B
%RTL8192ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_818910EC
%RTL8192ce.DeviceDesc%		= EDI8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_762210EC
%RTL8192ce.DeviceDesc%		= EDI8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_14001B9A
%RTL8192ce.DeviceDesc%		= EDI8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_14011B9A
%RTL8192ce.DeviceDesc%		= EDI8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_14021B9A
%RTL8192ce.DeviceDesc%		= ASUS8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_819010EC
%RTL8192ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_717810EC
%RTL8192ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_71791025
%RTL8192ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_71801025
%RTL8192ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_917810EC
%RTL8192ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_91791025
%RTL8192ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_91801025
%RTL8192ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_617810EC
%RTL8192ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_61791025
%RTL8192ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_61801025
%RTL8191ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8177
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_817610EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_817510EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_818110EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_818210EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_818410EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_818510EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821910EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820710EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820810EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820910EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821010EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_822010EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821110EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821210EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821310EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821410EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_822110EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821510EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821610EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821710EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_821810EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_822210EC
%RTL8188ce.DeviceDesc%		= SS8192Ce.ndi,		PCI\VEN_10EC&DEV_8176&SUBSYS_819110EC
%RTL8188ce.DeviceDesc%		= SS8192Ce.ndi,		PCI\VEN_10EC&DEV_8176&SUBSYS_819210EC
%RTL8188ce.DeviceDesc%		= SS8192Ce.ndi,		PCI\VEN_10EC&DEV_8176&SUBSYS_819310EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_11391A3B
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_81941028
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_819710EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_829710EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_38241462
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_81981028
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_8176185F
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820610EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_03151A32
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_7185144F
%HP8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_1629103C
%RTL8188ce.DeviceDesc%		= ASUS8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_819910EC
%RTL8188ce.DeviceDesc%		= ASUS8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820310EC
%RTL8188ce.DeviceDesc%		= ASUS8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820410EC
%RTL8188ce.DeviceDesc%		= ASUS8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_719510EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_23151A32
%RTL8188ce.DeviceDesc%		= EDI8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_761110EC
%RTL8188ce.DeviceDesc%		= INTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_818A10EC
%RTL8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_815010EC
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_717610EC
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_717710EC
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_717810EC
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_717910EC
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_718010EC
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_71811025
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_71821025
%RTL8188ceG.DeviceDesc%		= SSG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_719110EC
%RTL8188ceG.DeviceDesc%		= SSG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_719210EC
%RTL8188ceG.DeviceDesc%		= SSG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_719310EC
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_1A391A3B
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_824A1462
%RTL8188ceG.DeviceDesc%		= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_715010EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_917710EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_917610EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_917510EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_918110EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_918210EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_918410EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_918510EC
%HP8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_169F103C
%HP8188ce.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_1786103C
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_16B310CF
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_91861025
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_91871025
%RTL8188ceC.DeviceDesc%		= SS8192Ce.ndi,		PCI\VEN_10EC&DEV_8176&SUBSYS_919110EC
%RTL8188ceC.DeviceDesc%		= SS8192Ce.ndi,		PCI\VEN_10EC&DEV_8176&SUBSYS_919210EC
%RTL8188ceC.DeviceDesc%		= SS8192Ce.ndi,		PCI\VEN_10EC&DEV_8176&SUBSYS_919310EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_20571A3B
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_20781A3B
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_917410EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_919410EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_919610EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_91971028
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_38741462
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_91981028
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_920110EC
%RTL8188ceC.DeviceDesc%		= ASUS8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_920210EC
%RTL8188ceC.DeviceDesc%		= ASUS8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_920310EC
%RTL8188ceC.DeviceDesc%		= INTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_920510EC
%RTL8188ceC.DeviceDesc%		= RTL8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_915010EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_617610EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_617710EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_617810EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_617910EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_618010EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_61811025
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_61821025
%RTL8188ceCG.DeviceDesc%	= SSG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_619110EC
%RTL8188ceCG.DeviceDesc%	= SSG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_619210EC
%RTL8188ceCG.DeviceDesc%	= SSG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_619310EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_2A571A3B
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_874A1462
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_619410EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_619510EC
%RTL8188ceCG.DeviceDesc%	= RTLG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_615010EC
%RTL8188ce.DeviceDesc%		= XAVI8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_24811B9A
%RTL8188ce.DeviceDesc%  	= ACER8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_81861025
%RTL8188ce.DeviceDesc%  	= ACER8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_81871025
%RTL8188ce.DeviceDesc%  	= ACER8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_81301025
%RTL8188ce.DeviceDesc%  	= ACER8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_81311025
%RTL8192ce.DeviceDesc%  	= ACER8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_81791025
%RTL8192ce.DeviceDesc%  	= ACER8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_81801025
%RTL8188ce.DeviceDesc%  	= ACER8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_82301025
%RTL8188ce.DeviceDesc%  	= ACER8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_82311025
;;----------------------------------------------------------------------------
;; For 8192D RTK common
;;----------------------------------------------------------------------------
%RTL8192de0.DeviceDesc%		= RTL8192de0.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_819310EC&REV_00
%RTL8192de1.DeviceDesc%		= RTL8192de1.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_819310EC&REV_01
%RTL8192de0.DeviceDesc%		= RTL8192de0.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC&REV_00
%RTL8192de1.DeviceDesc%		= RTL8192de1.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC&REV_01
%RTL8192de0.DeviceDesc%		= RTL8192de0.ndi, 	PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA&REV_00
%RTL8192de1.DeviceDesc%		= RTL8192de1.ndi, 	PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA&REV_01
%RTL8192de0.DeviceDesc%		= RTL8192de0.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_01861025&REV_00
%RTL8192de1.DeviceDesc%		= RTL8192de1.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_01861025&REV_01
%RTL8192de0.DeviceDesc%		= RTL8192de0.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_929310EC&REV_00
%RTL8192de1.DeviceDesc%		= RTL8192de1.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_929310EC&REV_01
%RTL8192de0.DeviceDesc%		= RTL8192de0.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_829310EC&REV_00
%RTL8192de1.DeviceDesc%		= RTL8192de1.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_829310EC&REV_01
%RTL8192de0.DeviceDesc%		= RTL8192de0.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_819410EC&REV_00
%RTL8192de1.DeviceDesc%		= RTL8192de1.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_819410EC&REV_01
%RTL8192de0.DeviceDesc%		= RTL8192de0.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_819510EC&REV_00
%RTL8192de1.DeviceDesc%		= RTL8192de1.ndi, 	PCI\VEN_10EC&DEV_8193&SUBSYS_819510EC&REV_01
;;----------------------------------------------------------------------------
;; For 8723A RTK common
;;----------------------------------------------------------------------------
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_872310EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8724&SUBSYS_872410EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_872A&SUBSYS_872A10EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_872B&SUBSYS_872B10EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_072310EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_072410EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_07251025
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_072710EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_072810EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_072910EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_21141A3B	
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_073310EC
%RTL8723ae.DeviceDesc%		= RTL8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_073410EC
;;Asus
%RTL8723ae.DeviceDesc%		= ASUS8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_073010EC
%RTL8723ae.DeviceDesc%		= ASUS8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_073110EC
;;Clevo
%RTL8723ae.DeviceDesc%		= CLEVO8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_072610EC
;;Lenovo
%LNV8723ae.DeviceDesc%		= LNV8723ae.ndi,	PCI\VEN_10EC&DEV_8723&SUBSYS_073210EC
;;----------------------------------------------------------------------------
;; For 8188E RTK common
;;----------------------------------------------------------------------------
%RTL8188e.DeviceDesc%		= RTL8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_817910EC

;;LC
%RTL8188e.DeviceDesc%		= LC8188ee.ndi,		PCI\VEN_10EC&DEV_8179&SUBSYS_017917AA
%RTL8188e.DeviceDesc%		= LC8188ee.ndi,		PCI\VEN_10EC&DEV_8179&SUBSYS_019317AA
;;Acer
%RTL8188e.DeviceDesc%		= RTL8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_01801025
;;Toshiba
%RTL8188e.DeviceDesc%		= TSHB8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_018110EC
%RTL8188e.DeviceDesc%		= TSHB8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_018210EC
%RTL8188e.DeviceDesc%		= TSHB8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_018310EC
%RTL8188e.DeviceDesc%		= TSHB8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_018410EC
%RTL8188e.DeviceDesc%		= TSHB8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_018510EC
%RTL8188e.DeviceDesc%		= TSHB8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_018710EC
%RTL8188e.DeviceDesc%		= TSHB8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_019110EC
%RTL8188e.DeviceDesc%		= TSHB8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_019210EC
;;Clevo
%RTL8188e.DeviceDesc%		= CLV8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_018810EC
;;Intel
%RTL8188e.DeviceDesc%		= RTL8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_018910EC
;;HP
%HP8188e.DeviceDesc%		= HP8188ee.ndi,		PCI\VEN_10EC&DEV_8179&SUBSYS_197D103C
;;ASUS
%RTL8188e.DeviceDesc%		= ASUS8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_019010EC
;;AzureWave
%RTL8188e.DeviceDesc%		= AZW8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_1F381A3B
%RTL8188e.DeviceDesc%		= AZW8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_12381A3B
%RTL8188e.DeviceDesc%		= AZW8188ee.ndi,	PCI\VEN_10EC&DEV_8179&SUBSYS_1D381A3B

;;----------------------------------------------------------------------------
;; For 8812A RTK common
;;----------------------------------------------------------------------------
%RTL8812e.DeviceDesc%		= RTL8812e.ndi,		PCI\VEN_10EC&DEV_8812&SUBSYS_881210EC
%RTL8821e.DeviceDesc%		= RTL8821e.ndi,		PCI\VEN_10EC&DEV_8821&SUBSYS_882110EC

[Lenovo.NTamd64.6.0]
;;----------------------------------------------------------------------------
;; FOR 8192C LENOVO DEVICE DESC
;;----------------------------------------------------------------------------
%LNV8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_819510EC
%LNV8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820010EC
%LNV8188ce.DeviceDesc%		= LNVG8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_719410EC
%LNV8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_919510EC
%LNV8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_919910EC
%LNVC8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_920010EC
%LNVC8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_920410EC
%LNVC8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820110EC
%LNVC8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820210EC
%LNVC8188ce.DeviceDesc%		= LNV8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_820510EC

[ASUS.NTamd64.6.0]
;;----------------------------------------------------------------------------
;; FOR 8192C ASUS DEVICE DESC
;;----------------------------------------------------------------------------
%ASUSEdimax8188ce.DeviceDesc%	= ASED8192Ce.ndi,	PCI\VEN_10EC&DEV_8176&SUBSYS_84B51043
%ASUSEdimax8192ce.DeviceDesc%	= ASED8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_84B61043
[Edimax.NTamd64.6.0]
;;----------------------------------------------------------------------------
;; FOR 8192C Edimax DEVICE DESC
;;----------------------------------------------------------------------------
%RTL8192ce.DeviceDesc%		= EDI8192Ce.ndi,	PCI\VEN_10EC&DEV_8178&SUBSYS_76227392

;;****************************************************************************
;; Install
;;****************************************************************************
;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; Realtek G mode installation
;;----------------------------------------------------------------------------
[RTLG8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11gWirelessMode.reg, BTEnable.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTLG8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; Lenovo installation
;;----------------------------------------------------------------------------
[LNV8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg, ShowRxRate.reg, LPS.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LNV8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; Lenovo G mode installation
;;----------------------------------------------------------------------------
[LNVG8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11gWirelessMode.reg, BTEnable.reg, ShowRxRate.reg, LPS.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LNVG8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; SS installation
;;----------------------------------------------------------------------------
[SS8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg, RxWorkItem.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[SS8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; SS G Mode installation
;;----------------------------------------------------------------------------
[SSG8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11gWirelessMode.reg, BTEnable.reg, RxWorkItem.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[SSG8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; ASUS installation
;;----------------------------------------------------------------------------
[ASUS8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg, 11nAdhoc.reg, 11nTKIP.reg, 11nWEP.reg, ShowMaxRxRate.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASUS8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; ASED installation
;;----------------------------------------------------------------------------
[ASED8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg, 11nAdhoc.reg, 11nTKIP.reg, 11nWEP.reg, ShowMaxRxRate.reg, HWWPSPBC.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASED8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; EDI installation
;;----------------------------------------------------------------------------
[EDI8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg, HWWPSPBC.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[EDI8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; Intel installation
;;----------------------------------------------------------------------------
[INTL8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg, MinFwLPS.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[INTL8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; XAVI installation
;;----------------------------------------------------------------------------
[XAVI8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg, HWGPIO.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[XAVI8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; ACER installation
;;----------------------------------------------------------------------------
[ACER8192Ce.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, BTEnable.reg, WowlanEnableNoPatternMatch.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ACER8192Ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; Realtek Default installation
;;----------------------------------------------------------------------------
[RTL8192de0.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, EarlyModeEnable.reg, Chnl5G.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8192de0.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

[RTL8192de1.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, EarlyModeEnable.reg, Chnl5G.reg, ConcurrentMode.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8192de1.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; Realtek G Mode installation
;;----------------------------------------------------------------------------
[RTLG8192de0.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11gWirelessMode.reg, EarlyModeEnable.reg, Chnl5G.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTLG8192de0.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; Realtek Default installation
;;----------------------------------------------------------------------------
[RTL8723ae.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, FWLPSEnable.reg, 32kEnable.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8723ae.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

[ASUS8723ae.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, FWLPSEnable.reg, 32kEnable.reg, 11nAdhoc.reg, 11nTKIP.reg, 11nWEP.reg, ShowMaxRxRate.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASUS8723ae.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

[CLEVO8723ae.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, FWLPSEnable.reg, 32kEnable.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[CLEVO8723ae.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

[LNV8723ae.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, FWLPSEnable.reg, 32kEnable.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LNV8723ae.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8188ee.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, WowlanDisable.reg, 32kEnable.reg, DefaultAntennaAux.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8188ee.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; Toshiba installation
;;----------------------------------------------------------------------------
[TSHB8188ee.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, WowlanDisable.reg, 32kEnable.reg, DefaultAntennaAux.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[TSHB8188ee.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; LC installation
;;----------------------------------------------------------------------------
[LC8188ee.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, WowlanDisable.reg, 32kEnable.reg, DefaultAntennaAux.reg, ClearAMDWakeUpStatus.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LC8188ee.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; HP installation
;;----------------------------------------------------------------------------
[HP8188ee.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, WowlanDisable.reg, 32kEnable.reg, DefaultAntennaMain.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[HP8188ee.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; AzureWave installation
;;----------------------------------------------------------------------------
[AZW8188ee.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, WowlanDisable.reg, 32kEnable.reg, DefaultAntennaMain.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[AZW8188ee.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; Clevo installation
;;----------------------------------------------------------------------------
[CLV8188ee.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, WowlanDisable.reg, 32kEnable.reg, DefaultAntennaMain.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[CLV8188ee.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; ASUS installation
;;----------------------------------------------------------------------------
[ASUS8188ee.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11nWirelessMode.reg, WowlanDisable.reg, 32kEnable.reg, DefaultAntennaMain.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASUS8188ee.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8812e.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11acWirelessMode.reg, FWLPSEnable.reg, 32kDisable.reg, WowlanDisable.reg, EarlyModeEnable.reg, TcpReorderEnable.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8812e.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8821e.ndi.NT]
AddReg          = NDIS_60.reg, RTLWLAN.reg, 11acWirelessMode.reg, FWLPSEnable.reg, 32kDisable.reg, WowlanDisable.reg, EarlyModeEnable.reg, TcpReorderEnable.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8821e.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog

;;****************************************************************************
;; OS relative registry
;;****************************************************************************
;;----------------------------------------------------------------------------
;; NDIS Common Parameters
;;----------------------------------------------------------------------------
[NDIS_60.reg]
HKR, Ndi,                       Service,    0, "RTWlanE"
HKR, Ndi\Interfaces,		UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,		LowerRange, 0, "wlan,ethernet"

;;----------------------------------------------------------------------------
;; RTWLAN Common Parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,			AH_BcnIntv, 	0, "1000"
HKR,Ndi\params\AH_BcnIntv, 	default, 	0, "100"
HKR,Ndi\params\AH_BcnIntv,	ParamDesc, 	0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, 	type, 		0, "int"
HKR,Ndi\params\AH_BcnIntv, 	min, 		0, "20"
HKR,Ndi\params\AH_BcnIntv, 	max, 		0, "1000"
HKR,Ndi\params\AH_BcnIntv, 	step, 		0, "1"

HKR,Ndi\params\Dot11dEnable,        ParamDesc,  0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable,        type,       0, "enum"
HKR,Ndi\params\Dot11dEnable,        default,    0, "0"
HKR,Ndi\params\Dot11dEnable\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"

;Roaming Sensitivity Level
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, %ROAMING_SENSITIVITY_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "80"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127",  0, %DISABLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "65",  0, %HIGH_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70",  0, %MIDDLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80",  0, %LOW_STR%

HKR,Ndi\params\PreambleMode,        ParamDesc,  0, %PREAMBLE_MODE_STR%
HKR,Ndi\params\PreambleMode,        type,       0, "enum"
HKR,Ndi\params\PreambleMode,        default,    0, "2"
HKR,Ndi\params\PreambleMode\enum,   "1",        0, %LONG_PREAMBLE_STR%
HKR,Ndi\params\PreambleMode\enum,   "2",        0, %LONG_SHORT_PREAMBLE_STR%
HKR,defaults,PreambleMode,0,"2"
HKR,,PreambleMode,0,"2"

;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\WiFiConfg,        ParamDesc,  0, "WiFi Config"
HKR,Ndi\params\WiFiConfg,        type,       0, "enum"
HKR,Ndi\params\WiFiConfg,        default,    0, "0"
HKR,Ndi\params\WiFiConfg\enum,   "0",        0, "Performance"
HKR,Ndi\params\WiFiConfg\enum,   "1",        0, "WiFi"
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"
HKR,,WiFiConfg,,"0"

;; 40MHz Support in 11n
HKR,Ndi\params\BW40MHz,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BW40MHz,        type,       0, "enum"
HKR,Ndi\params\BW40MHz,        default,    0, "1"
HKR,Ndi\params\BW40MHz\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHz\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHz,0,"1"
HKR,,BW40MHz,0,"1"
HKR,,BW40MHz,,"1"

HKR,,Channel,0,"10"

;Inactive Power Save
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;; RF Off
;HKR,defaults,HwSwRfOffD3,0,"0"
HKR,,HwSwRfOffD3,0,"0"

;; ASPM
HKR,defaults,PciASPM,0,"5"
HKR,,PciASPM,0,"5"

;Keep Alive Mechanism
HKR,,KeepAliveLevel,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

HKR,defaults,BINumber,0,"10"
HKR,,BINumber,0,"10"

;;----------------------------------------------------------------------------
;; Wireless Mode Related Parameters
;;----------------------------------------------------------------------------
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

[11acWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "64"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"64", 		0, %IEEE_802_11ANAC_STR%
HKR,defaults,WirelessMode, 0, "64"
HKR,,WirelessMode, 0, "64"

HKR,defaults,BW40MHz,0,"1"
HKR,,BW40MHz,0,"1"

HKR,defaults,BW80MHz,0,"1"
HKR,,BW80MHz,0,"1"

;;----------------------------------------------------------------------------
;; ADHOC Related Parameters
;;----------------------------------------------------------------------------
[11nAdhoc.reg]
HKR,Ndi\params\11nAdhoc,        ParamDesc,  0, %11NADHOC_ENABLE_STR%
HKR,Ndi\params\11nAdhoc,        type,       0, "enum"
HKR,Ndi\params\11nAdhoc,        default,    0, "0"
HKR,Ndi\params\11nAdhoc\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\11nAdhoc\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,11nAdhoc,0,"0"
HKR,,11nAdhoc,0,"0"

;;----------------------------------------------------------------------------
;; BT Control Parameters
;;----------------------------------------------------------------------------
[BTEnable.reg]
HKR,,bBTMode,0,"1"
[BTDisable.reg]
HKR,,bBTMode,0,"0"

;;----------------------------------------------------------------------------
;; MSI Control Parameters
;;----------------------------------------------------------------------------
[MSIEnable.reg]
HKR,,MSISupport,0,"1"
[MSIDisable.reg]
HKR,,MSISupport,0,"0"

;;----------------------------------------------------------------------------
;; WOWLAN Control Parameters
;;----------------------------------------------------------------------------
[WowlanAllEnable.reg]
HKR,,WoWLANMode,0,"3"
HKR,,WoWLANLPSLevel,0,"1"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanDisable.reg]
HKR,,WoWLANMode,0,"0"
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"0"
HKR,,GTKOffloadEnable,0,"0"

[WowlanAllEnableNoLPS.reg]
HKR,,WoWLANMode,0,"3"
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanEnableNoPatternMatch.reg]
HKR,,WoWLANMode,0,"1"
HKR,,WoWLANLPSLevel,0,"1"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "0"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanEnableNoLPSNoPatternMatch.reg]
HKR,,WoWLANMode,0,"1"
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "0"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%
;;----------------------------------------------------------------------------
;; Earlymode Control Parameters
;;----------------------------------------------------------------------------
[EarlyModeEnable.reg]
HKR,,bEarlymodeEnable,0,"1"
[EarlyModeDisable.reg]
HKR,,bEarlymodeEnable,0,"0"

;;----------------------------------------------------------------------------
;; LPS Control Parameters
;;----------------------------------------------------------------------------
[FWLPSEnable.reg]
HKR,,bFwCtrlLPS,0,"1"
[FWLPSDisable.reg]
HKR,,bFwCtrlLPS,0,"0"

;;----------------------------------------------------------------------------
;; LPS 32k Control Parameters
;;----------------------------------------------------------------------------
[32kEnable.reg]
HKR,,bLowPowerEnable,0,"1"
[32kDisable.reg]
HKR,,bLowPowerEnable,0,"0"

;;----------------------------------------------------------------------------
;; TxPowerTracking Control Parameters
;;----------------------------------------------------------------------------
[PowerTrackingCtr.reg]
HKR,,PowerTrackingSupport,,"1"
HKR,,PowerTrackingIQKSupport,,"1"

;;----------------------------------------------------------------------------
;; TCP Reorder Control Parameters
;;----------------------------------------------------------------------------
[TcpReorderEnable.reg]
HKR,,TcpReorder,0,"1"
[TcpReorderDisable.reg]
HKR,,TcpReorder,0,"0"

;;----------------------------------------------------------------------------
;; Default Antenna Control Parameters
;;----------------------------------------------------------------------------
[DefaultAntennaMain.reg]
HKR,,bRegDefaultAntenna,0,"1"
[DefaultAntennaAux.reg]
HKR,,bRegDefaultAntenna,0,"0"

;;----------------------------------------------------------------------------
;; Clear AMD PCIE WAKE UP Status and PME wake up status
;;----------------------------------------------------------------------------
[ClearAMDWakeUpStatus.reg]
HKR,,ClearAMDWakeUpStatus,0,"1"

;;----------------------------------------------------------------------------
;; RTL8192ce Special Parameters
;;----------------------------------------------------------------------------
[LPS.reg]
HKR,Ndi\params\bLeisurePs,        ParamDesc,  0, %LEISURE_POWER_SAVE_STR%
HKR,Ndi\params\bLeisurePs,        type,       0, "enum"
HKR,Ndi\params\bLeisurePs,        default,    0, "2"
HKR,Ndi\params\bLeisurePs\enum,   "2",        0, %LEISURE_POWER_SAVE_AUTO%
HKR,Ndi\params\bLeisurePs\enum,   "0",        0, %LEISURE_POWER_SAVE_DISABLE%
HKR,Ndi\params\bLeisurePs\enum,   "1",        0, %LEISURE_POWER_SAVE_ENABLE%

[ShowRxRate.reg]
HKR,,ShowRate,0,"2"

[RxWorkItem.reg]
HKR,,UseRxInterruptWorkItem,0,"1"

[ShowMaxRxRate.reg]
HKR,,ShowRate,0,"3"

[11nTKIP.reg]
HKR,,TKIPinNmode,0,"1"

[11nWEP.reg]
HKR,,WEPinNmode,0,"1"

[HWWPSPBC.reg]
HKR,,GPIORFSW,0,"0"
HKR,,GPIOHWPBC,0,"1"

[HWGPIO.reg]
HKR,,GPIORFSW,0,"1"
HKR,,GPIOHWPBC,0,"1"

[MinFwLPS.reg]
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

[Intel.reg]
HKR,Ndi\params\ForcedBstDataRate,        ParamDesc,  0, "Broadcast/Multicast Data Rate"
HKR,Ndi\params\ForcedBstDataRate,        type,       0, "enum"
HKR,Ndi\params\ForcedBstDataRate,        default,    0, "0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "0",        0, "Auto"
HKR,Ndi\params\ForcedBstDataRate\enum,   "2",        0, "1Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "4",        0, "2Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "11",      0, "5.5Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "22",     0, "11Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "12",      0, "6Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "18",     0, "9Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "24",     0, "12Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "36",     0, "18Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "48",     0, "24Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "72",     0, "36Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "96",     0, "48Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "108",     0, "54Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "128",     0, "MCS0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "129",     0, "MCS1"
HKR,Ndi\params\ForcedBstDataRate\enum,   "130",     0, "MCS2"
HKR,Ndi\params\ForcedBstDataRate\enum,   "131",     0, "MCS3"
HKR,Ndi\params\ForcedBstDataRate\enum,   "132",     0, "MCS4"
HKR,Ndi\params\ForcedBstDataRate\enum,   "133",     0, "MCS5"
HKR,Ndi\params\ForcedBstDataRate\enum,   "134",     0, "MCS6"
HKR,Ndi\params\ForcedBstDataRate\enum,   "135",     0, "MCS7"
HKR,Ndi\params\ForcedBstDataRate\enum,   "136",     0, "MCS8"
HKR,Ndi\params\ForcedBstDataRate\enum,   "137",     0, "MCS9"
HKR,Ndi\params\ForcedBstDataRate\enum,   "138",     0, "MCS10"
HKR,Ndi\params\ForcedBstDataRate\enum,   "139",     0, "MCS11"
HKR,Ndi\params\ForcedBstDataRate\enum,   "140",     0, "MCS12"
HKR,Ndi\params\ForcedBstDataRate\enum,   "141",     0, "MCS13"
HKR,Ndi\params\ForcedBstDataRate\enum,   "142",     0, "MCS14"
HKR,Ndi\params\ForcedBstDataRate\enum,   "143",     0, "MCS15"
;;----------------------------------------------------------------------------
;; RTL8192de Special Parameters
;;----------------------------------------------------------------------------
[Chnl5G.reg]
HKR,,Channel5G,0,"36"

[Mac0Vwifi.reg]
HKR,,MAC0VWifiSupport,0,"0"

[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode,		ParamDesc,  0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode,		type,       0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode,			default,    0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"0",        0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"1",        0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"2",        0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"


;;****************************************************************************
;; OS relative service.
;;****************************************************************************
[RTWlanE.Service]
DisplayName     = %RTWlanE.DeviceDesc.DispName%
ServiceType     = 1 		;SERVICE_KERNEL_DRIVER
StartType       = 3 		;SERVICE_DEMAND_START
ErrorControl    = 1 		;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\rtwlane.sys
LoadOrderGroup  = NDIS

[RTWlanE.EventLog]
AddReg = RTWlanE.AddEventLog.reg

[RTWlanE.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[RTWlanE.CopyFiles]
rtwlane.sys,,,2


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
RTWlanE.CopyFiles        = 12
DefaultDestDir             = 11        ; LDID_SYS
CIHVS.CopyFiles					= 11
RtlUI2.CopyFiles				= 10

;;****************************************************************************
;; Source Files
;;****************************************************************************
[CIHVS.CopyFiles]
Rtlihvs.dll,,,2
RtlEXTUI.DLL,,,2

[RegisterUIExt]
11,,RtlExtUI.dll,1

[RtlUI2.CopyFiles]
RtlUI2.exe,,,2

[SourceDisksNames]
1 = %DISKNAME%,,,

[SourceDisksFiles]
rtwlane.sys = 1
Rtlihvs.dll = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek     				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR 			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"

TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
CHANNEL_PLAN_STR			= "Channel Plan"
WL_MODE_STR				= "Wireless Mode"
PREAMBLE_MODE_STR			= "Preamble Mode"
FRAGTHRESH_STR				= "Fragmentation Threshold"
RTSTHRESH_STR				= "RTS Threshold"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Disabled"
ENABLE_STR 				= "Enabled"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Auto select"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR		= "Leisure Power Save"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"			

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0009] ; English
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR 			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
CHANNEL_PLAN_STR			= "Channel Plan"
WL_MODE_STR				= "Wireless Mode"
PREAMBLE_MODE_STR			= "Preamble Mode"
FRAGTHRESH_STR				= "Fragmentation Threshold"
RTSTHRESH_STR				= "RTS Threshold"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Disabled"
ENABLE_STR 				= "Enabled"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Auto select"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
SHORT_PREAMBLE_STR 			= "Short Preamble"
LONG_SHORT_PREAMBLE_STR			= "Short & long"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR			= "Leisure Power Save"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "25 %"			

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0404] ; Chinese (Traditional)
Realtek					= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "服務組合識別碼"
CHANNEL_STR				= "通訊頻道"
NETWORK_TYPE_STR 			= "無線網路操作模式"
LED_CONTROL_STR				= "驅動程式控制 LED 閃爍模式" 
POWER_SAVE_STR				= "省電模式"
WIFI_IBSS_STR				= "對等式網路只使用 802.11b 標準"
RATE_ADAPTIVE_STR			= "適應性傳輸率調變自動化模式"
QOS_STR					= "流量管控"
WMM_APSD				= "WiFi 多媒體自動化省電參數 (WMM APSD)"
CCX_RM_STR				= "CCX 無線網路環境監控"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 非連線頻道最大量測時間 (0: 無限大)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "支援 PSP XLink 連線模式"
CHANNEL_PLAN_STR			= "頻道規劃"
WL_MODE_STR				= "無線網路標準"
PREAMBLE_MODE_STR			= "前序訊號模式"
FRAGTHRESH_STR				= "區段臨界值"
RTSTHRESH_STR				= "RTS 臨界值"
DOT11_ENABLE_STR			= "802.11d 無線頻道區域規範"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "啟用"
CAM_STR 				= "無"
MAX_PSP_STR 				= "最大"
FAST_PSP_STR 				= "最小"
AD_HOC_STR 				= "對等式網路"
INFRASTRUCTURE_STR 			= "主從式網路"
AUTO_SELECT_STR 			= "自動選擇"
DOMAIN_FROM_EEPROM_STR 			= "硬體決定"
AUTO_STR 				= "自動選擇"
LONG_PREAMBLE_STR 			= "唯獨長前序訊號"
SHORT_PREAMBLE_STR 			= "短前序訊號"
LONG_SHORT_PREAMBLE_STR			= "長與短前序訊號"

FCC_STR 				= "FCC"

IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "漫遊重試限制（秒）"
LEISURE_POWER_SAVE_STR			= "空閒電力節省"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "信標間隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "25 %"			

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0011] ; Japanese
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "チャンネル"
NETWORK_TYPE_STR 			= "ネットワークの種類"
LED_CONTROL_STR				= "LEDコントロール" 
POWER_SAVE_STR				= "省電力モード"
WIFI_IBSS_STR				= "IBSS既定11bモード"
RATE_ADAPTIVE_STR			= "適応レート"
QOS_STR					= "QoS "
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCXラジオ測定"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX最大オフライン測定（0: 無制限）"
FORCE_PRIORITY_STR			= "強制実行優先順位"
HW_PARA_STR				= "HwParaFileからのInit "
THREE_WIRE_MODE_STR			= "三線式プログラミングモード"
BOARD_TYPE_STR				= "基板の種類"
PROTECTION_MODE_STR			= "保護モード"
TPC_STR					= "送信電力制御"
TPC_POLARITY_STR			= "TPC極性選択"
HIGH_POWER_STR				= "高出力機構"
INIT_GAIN_STR				= "初期ゲイン状態"
CW_MAX_MIN_STR				= "コンテンションウィンドウ"
PSP_XLINK_STR				= "PSP XLinkモード"
CHANNEL_PLAN_STR			= "チャンネルプラン"
WL_MODE_STR				= "ワイヤレスモード"
PREAMBLE_MODE_STR			= "プレアンブルモード"
FRAGTHRESH_STR				= "フラグメンテーションしきい値"
RTSTHRESH_STR				= "RTSしきい値"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "無効"
ENABLE_STR 				= "有効"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "臨時"
INFRASTRUCTURE_STR 			= "インフラストラクチャ"
AUTO_SELECT_STR 			= "自動選択"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "自動"
LONG_PREAMBLE_STR 			= "長いプリアンブル"
SHORT_PREAMBLE_STR 			= "短いプリアンブル"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "スペイン"
FRANCE_STR 				= "フランス"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "イスラエル"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "ローミング再試行制限 (秒)"
LEISURE_POWER_SAVE_STR			= "レジャーパワーセーブ"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "ビーコン間隔"


ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "25 %"			

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0007] ; German
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Netzwerktyp"
LED_CONTROL_STR				= "LED-Anzeige" 
POWER_SAVE_STR				= "Energiesparmodus"
WIFI_IBSS_STR				= "IBSS Default 11b Modus"
RATE_ADAPTIVE_STR			= "Ratenadaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Funkmessung"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max. Offline Messung (0: unbeschrankt)"
FORCE_PRIORITY_STR			= "Erzwungene Prioritat"
HW_PARA_STR				= "Init. von HwParaFile"
THREE_WIRE_MODE_STR			= "Dreileiter-Programmiermodus"
BOARD_TYPE_STR				= "Kartentyp"
PROTECTION_MODE_STR			= "Schutzmodus"
TPC_STR					= "Ubertragungsleistungsstuerung"
TPC_POLARITY_STR			= "TPC Polaritatsauswahl"
HIGH_POWER_STR				= "Hochleistungsmechanismus"
INIT_GAIN_STR				= "Anfangl. Verstarkungszustand"
CW_MAX_MIN_STR				= "Konkurrenz-Fenster"
PSP_XLINK_STR				= "PSP XLink Modus"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Wireless-Modus"
PREAMBLE_MODE_STR			= "Praambelmodus"
FRAGTHRESH_STR				= "Fragmentierungsschwelle"
RTSTHRESH_STR				= "RTS-Schwelle:"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktivieren"
ENABLE_STR 				= "Aktivieren"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autom. Auswahl"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lange Praambel"
SHORT_PREAMBLE_STR 			= "Kurze Praambel"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankreich"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roaming-Wiederholungslimit (Sek.)"
LEISURE_POWER_SAVE_STR			= "Leerlauf-Energiesparen"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Bakenintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.000c] ; French
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Type de reseau"
LED_CONTROL_STR				= "Commande DEL" 
POWER_SAVE_STR				= "Mode economie d'energie"
WIFI_IBSS_STR				= "Mode 11b par defaut IBSS"
RATE_ADAPTIVE_STR			= "Debit adaptable"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Mesure radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Mesure hors ligne max. (0: illimitee)"
FORCE_PRIORITY_STR			= "Priorite forcee"

HW_PARA_STR				= "Init de HwParaFile"
THREE_WIRE_MODE_STR			= "Mode de programmation trois fils"
BOARD_TYPE_STR				= "Type de carte"
PROTECTION_MODE_STR			= "Mode de protection"
TPC_STR					= "Transmission du reglage"
TPC_POLARITY_STR			= "Choix de la polarite TPC"
HIGH_POWER_STR				= "Mecanisme grande puissance"
INIT_GAIN_STR				= "Etat du gain initial"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "Mode XLink PSP"
CHANNEL_PLAN_STR			= "Plan de canal"
WL_MODE_STR				= "Mode sans fil"
PREAMBLE_MODE_STR			= "Mode preambule"
FRAGTHRESH_STR				= "Seuil de fragmentation"
RTSTHRESH_STR				= "Seuil RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Desactiver"
ENABLE_STR 				= "Activer"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Selection automatique"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "preambule long"
SHORT_PREAMBLE_STR 			= "Preambule court"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espagne"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite essais roam (sec)"
LEISURE_POWER_SAVE_STR			= "Economie d'energie loisirs"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Intervalle balise "

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0010] ; Italian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Canale"
NETWORK_TYPE_STR 			= "Tipo di rete"
LED_CONTROL_STR				= "Controllo LED" 
POWER_SAVE_STR				= "Modalita risparmio energetico"
WIFI_IBSS_STR				= "Modalita IBBS predefinita 11b"
RATE_ADAPTIVE_STR			= "Si adatta alla velocita"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Misurazione radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Misurazione CCD max non in linea (0: illimitata)"
FORCE_PRIORITY_STR			= "Priorita forzata"
HW_PARA_STR				= "Init da HwParaFile"
THREE_WIRE_MODE_STR			= "Tre modalita di programmazione cablata"
BOARD_TYPE_STR				= "Tipo di piastra"

PROTECTION_MODE_STR			= "Modalita protezione"
TPC_STR					= "Trasmissione risparmio energetico"
TPC_POLARITY_STR			= "Selezione della polarita TPC"
HIGH_POWER_STR				= "Meccanismo ad alto potenziale"
INIT_GAIN_STR				= "Stato di guadagno iniziale"
CW_MAX_MIN_STR				= "Finestra di competizione"
PSP_XLINK_STR				= "Modalita PSP XLink"
CHANNEL_PLAN_STR			= "Piano canale"
WL_MODE_STR				= "Modalita wireless"
PREAMBLE_MODE_STR			= "Modalita preambolo"
FRAGTHRESH_STR				= "Soglia di frammentazione"
RTSTHRESH_STR				= "Soglia RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Disabilita"
ENABLE_STR 				= "Abilita"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruttura"
AUTO_SELECT_STR 			= "Selezione automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Preambolo lungo"
SHORT_PREAMBLE_STR 			= "Preambolo breve"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spagna"
FRANCE_STR 				= "Francia"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israele"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite tentativi roam (sec)"
LEISURE_POWER_SAVE_STR			= "Risparmio energetico tempo libero"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.000a] ; Spanish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Tipo de red"
LED_CONTROL_STR				= "Control de LED" 
POWER_SAVE_STR				= "Modo de ahorro de energia"
WIFI_IBSS_STR				= "Modo 11b predeterminado IBSS"
RATE_ADAPTIVE_STR			= "Velocidad adaptable"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Medicion de radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medicion sin conexion maxima CCX (0: sin limite)"
FORCE_PRIORITY_STR			= "Prioridad forzada"
HW_PARA_STR				= "Inicio desde HwParaFile"
THREE_WIRE_MODE_STR			= "Modo de programacion de tres cables"
BOARD_TYPE_STR				= "Tipo de tablero"
PROTECTION_MODE_STR			= "Modo de proteccion"
TPC_STR					= "Transmitir control de potencia"
TPC_POLARITY_STR			= "Seleccionar polaridad TPC"
HIGH_POWER_STR				= "Mecanismo de alta potencia"
INIT_GAIN_STR				= "Estado de ganancia inicial"
CW_MAX_MIN_STR				= "Ventana de discusiones"
PSP_XLINK_STR				= "Modo XLink PSP"
CHANNEL_PLAN_STR			= "Plan de canal"
WL_MODE_STR				= "Modo inalambrico"
PREAMBLE_MODE_STR			= "Modo de preambulo"
FRAGTHRESH_STR				= "Umbral de fragmentacion"
RTSTHRESH_STR				= "Umbral RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deshabilitar"
ENABLE_STR 				= "Habilitar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "PSP_rapido"
AD_HOC_STR 				= "Especial"
INFRASTRUCTURE_STR 			= "Infraestructura"
AUTO_SELECT_STR 			= "Seleccion automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMINIO_DE_EEPROM"
AUTO_STR 				= "Automatico"
LONG_PREAMBLE_STR 			= "Preambulo largo"
SHORT_PREAMBLE_STR 			= "Preambulo corto"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espana"
FRANCE_STR 				= "Francia"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite de reintentos en transito (seg)"
LEISURE_POWER_SAVE_STR			= "Ahorro de energia por inactividad"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Intervalo de baliza"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0c04] ; Chinese (Traditional) (Hong Kong)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR				= "服務組合識別碼"
CHANNEL_STR				= "通訊頻道"
NETWORK_TYPE_STR			= "無線網路操作模式"
LED_CONTROL_STR				= "驅動程式控制 LED 閃爍模式" 
POWER_SAVE_STR				= "省電模式"
WIFI_IBSS_STR				= "對等式網路只使用 802.11b 標準"
RATE_ADAPTIVE_STR			= "適應性傳輸率調變自動化模式"
QOS_STR					= "流量管控"
WMM_APSD				= "WiFi 多媒體自動化省電參數 (WMM APSD)"
CCX_RM_STR				= "CCX 無線網路環境監控"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 非連線頻道最大量測時間 (0: 無限大)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "支援 PSP XLink 連線模式"
CHANNEL_PLAN_STR			= "頻道規劃"
WL_MODE_STR				= "無線網路標準"
PREAMBLE_MODE_STR			= "前序訊號模式"
FRAGTHRESH_STR				= "區段臨界值"
RTSTHRESH_STR				= "RTS 臨界值"
DOT11_ENABLE_STR			= "802.11d 無線頻道區域規範"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "啟用"
CAM_STR 				= "無"
MAX_PSP_STR 				= "最大"
FAST_PSP_STR 				= "最小"
AD_HOC_STR 				= "對等式網路"
INFRASTRUCTURE_STR 			= "主從式網路"
AUTO_SELECT_STR 			= "自動選擇"
DOMAIN_FROM_EEPROM_STR 			= "硬體決定"
AUTO_STR 				= "自動選擇"
LONG_PREAMBLE_STR 			= "長前序訊號"
SHORT_PREAMBLE_STR 			= "短前序訊號"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "漫遊重試上限（秒）"
LEISURE_POWER_SAVE_STR			= "閑置中電源管理"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "信標間隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0804] ; Chinese (Simplified)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "频道"
NETWORK_TYPE_STR 			= "网络类型"
LED_CONTROL_STR				= "LED 控制" 
POWER_SAVE_STR				= "省电模式"
WIFI_IBSS_STR				= "IBSS 默认 11b 模式"
RATE_ADAPTIVE_STR			= "速率适应"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX 无线电测量"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 最大脱机测量（0：无限制）"
FORCE_PRIORITY_STR			= "强制优先级"
HW_PARA_STR				= "从硬件参数文件初始化"
THREE_WIRE_MODE_STR			= "三线编程模式"
BOARD_TYPE_STR				= "板子类型"
PROTECTION_MODE_STR			= "保护模式"
TPC_STR					= "发射功率控制"
TPC_POLARITY_STR			= "TPC 极性选择"
HIGH_POWER_STR				= "高功率机制"
INIT_GAIN_STR				= "初始增益状态"
CW_MAX_MIN_STR				= "争用窗口"
PSP_XLINK_STR				= "PSP XLink 模式"
CHANNEL_PLAN_STR			= "频道计划"
WL_MODE_STR				= "无线模式"
PREAMBLE_MODE_STR			= "前导码模式"
FRAGTHRESH_STR				= "碎片阈值"
RTSTHRESH_STR				= "RTS 阈值"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "启用"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "对等网络"
INFRASTRUCTURE_STR 			= "基础架构"
AUTO_SELECT_STR 			= "自动选择"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "自动"
LONG_PREAMBLE_STR 			= "长前导码"
SHORT_PREAMBLE_STR 			= "短前导码"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "西班牙"
FRANCE_STR 				= "法国"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "以色列"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "漫游重试限制(秒)"
LEISURE_POWER_SAVE_STR			= "空闲省电"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "信标间隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0012] ; Korean
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR				= "SSID"
CHANNEL_STR				= "채널"
NETWORK_TYPE_STR			= "네트워크 종류"
LED_CONTROL_STR				= "LED 제어" 
POWER_SAVE_STR				= "절전 모드"
WIFI_IBSS_STR				= "IBSS 기본 11b 모드"

RATE_ADAPTIVE_STR			= "속도 적응"
QOS_STR					= " QoS "
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX 무선 측정"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 최대 오프라인 측정(0: 제한 없음)"
FORCE_PRIORITY_STR			= "강제 우선 순위"
HW_PARA_STR				= "HwParaFile에서 초기화"
THREE_WIRE_MODE_STR			= "3선 식 프로그래밍 모드"
BOARD_TYPE_STR				= "보드 종류"
PROTECTION_MODE_STR			= "보호 모드"

TPC_STR					= "송신 출력 제어"
TPC_POLARITY_STR			= "TPC 극성 선택"
HIGH_POWER_STR				= "고출력 메커니즘"
INIT_GAIN_STR				= "초기 게인 상태"
CW_MAX_MIN_STR				= "경합 창"
PSP_XLINK_STR				= "PSP XLink 모드"

CHANNEL_PLAN_STR			= "채널 계획"
WL_MODE_STR				= "무선 모드"
PREAMBLE_MODE_STR			= "프리앰블 모드"
FRAGTHRESH_STR 				= "조각화 임계값"
RTSTHRESH_STR				= "RTS 임계값"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "사용 안 함"
ENABLE_STR 				= "사용"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "애드혹"
INFRASTRUCTURE_STR 			= "인프라"
AUTO_SELECT_STR 			= "자동 선택"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "자동"
LONG_PREAMBLE_STR 			= "긴 프리앰블"
SHORT_PREAMBLE_STR 			= "짧은 프리앰블"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "스페인"
FRANCE_STR 				= "프랑스"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "이스라엘"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "로밍 재시도 제한시간(초)"
LEISURE_POWER_SAVE_STR			= "대기 절전"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "비컨 간격"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0816] ; Portuguese (Portugal)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Tipo de rede"
LED_CONTROL_STR				= "Controlo dos LEDs" 
POWER_SAVE_STR				= "Modo de poupanca de energia"
WIFI_IBSS_STR				= "Modo IBSS 11b predefinido"
RATE_ADAPTIVE_STR			= "Velocidade adaptativa"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Medida de radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medida off-line maxima CCX (0: ilimitada)"
FORCE_PRIORITY_STR			= "Prioridade forcada"
HW_PARA_STR				= "Iniciar a partir de ficheiro de parametros do hardware"
THREE_WIRE_MODE_STR			= "Modo de programacao com tres fios"
BOARD_TYPE_STR				= "Tipo de placa"
PROTECTION_MODE_STR			= "Modo de proteccao"
TPC_STR					= "Controlo da potencia de transmissao"
TPC_POLARITY_STR			= "Seleccao da polaridade TPC"
HIGH_POWER_STR				= "Mecanismo de alta potencia"
INIT_GAIN_STR				= "Estado de ganho inicial"
CW_MAX_MIN_STR				= "Janela de contencao"
PSP_XLINK_STR				= "Modo PSP XLink"
CHANNEL_PLAN_STR			= "Plano de canais"
WL_MODE_STR				= "Modo sem fios"
PREAMBLE_MODE_STR			= "Modo de preambulo"
FRAGTHRESH_STR				= "Limiar de fragmentacao"
RTSTHRESH_STR				= "Limiar RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Desactivar"
ENABLE_STR 				= "Activar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infraestrutura"
AUTO_SELECT_STR 			= "Seleccao automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMINIO_DE_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Preambulo longo"
SHORT_PREAMBLE_STR 			= "Preambulo curto"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanha"
FRANCE_STR 				= "Franca"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite para tentativas de itinerancia (seg.)"
LEISURE_POWER_SAVE_STR			= "Poupanca de energia em diversao"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Intervalo de sinalizacao"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0013] ; Dutch
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanaal"
NETWORK_TYPE_STR 			= "Netwerktype"
LED_CONTROL_STR				= "LED-besturing" 
POWER_SAVE_STR				= "Spaarstandmodus"
WIFI_IBSS_STR				= "IBSS standaard 11b-modus"
RATE_ADAPTIVE_STR			= "Aanpasbare snelheid"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX-radiometing"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX max. verschuivingsmeting (0: onbeperkt)"
FORCE_PRIORITY_STR			= "Geforceerde prioriteit"
HW_PARA_STR				= "Init van HwParaFile"
THREE_WIRE_MODE_STR			= "Driedraads programmeermodus"
BOARD_TYPE_STR				= "Bordtype"
PROTECTION_MODE_STR			= "Beveiligingsmodus"
TPC_STR					= "Zendvermogenbeheer"
TPC_POLARITY_STR			= "Selectie TPC-polariteit"

HIGH_POWER_STR				= "Mechanisme met hoog vermogen"
INIT_GAIN_STR				= "Eerste versterkingsstatus"
CW_MAX_MIN_STR				= "Conflictvenster"
PSP_XLINK_STR				= "PSP XLink-modus"
CHANNEL_PLAN_STR			= "Kanaalplan"
WL_MODE_STR				= "Draadloze modus"
PREAMBLE_MODE_STR			= "Preambulemodus"
FRAGTHRESH_STR				= "Fragmentatiedrempel"
RTSTHRESH_STR				= "RTS-drempel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Uitschakelen"
ENABLE_STR 				= "Inschakelen"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad hoc"
INFRASTRUCTURE_STR 			= "Infrastructuur"
AUTO_SELECT_STR 			= "Auto selectie"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lange preambule"
SHORT_PREAMBLE_STR 			= "Korte preambule"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanje"
FRANCE_STR 				= "Frankrijk"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limiet van roamingspogingen(sec)"
LEISURE_POWER_SAVE_STR			= "Energiebesparing"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Bakeninterval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0014] ; Norwegian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Nettverkstype"
LED_CONTROL_STR				= "LED-kontroll" 
POWER_SAVE_STR				= "Stromsparingsmodus"
WIFI_IBSS_STR				= "IBSS standard 11b-modus"
RATE_ADAPTIVE_STR			= "Hastighet adaptiv"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radiomaling"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX maks offline-maling (0: ubegrenset)"
FORCE_PRIORITY_STR			= "Tvunget prioritet"
HW_PARA_STR				= "Init fra HwParaFile"
THREE_WIRE_MODE_STR			= "Tre tradet programmeringsmodus"
BOARD_TYPE_STR				= "Korttype"
PROTECTION_MODE_STR			= "Beskyttelsesmodus"
TPC_STR					= "Stromsendingskontroll"
TPC_POLARITY_STR			= "Velg TPC-polaritet"
HIGH_POWER_STR				= "Hoystyrke-mekanisme"
INIT_GAIN_STR				= "Opprinnelig okningstilstand"
CW_MAX_MIN_STR				= "Konflikt-vindu"
PSP_XLINK_STR				= "PSP XLink-modus"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Tradlos modus"
PREAMBLE_MODE_STR			= "Innledende modus"
FRAGTHRESH_STR				= "Fragmenteringsgrense"
RTSTHRESH_STR				= "RTS-grense"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktiver"
ENABLE_STR 				= "Aktiver"
CAM_STR 				= "KAM"
MAX_PSP_STR 				= "MAKS_PSP"
FAST_PSP_STR 				= "Rask_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autovelg"
DOMAIN_FROM_EEPROM_STR 			= "DOMENE_FRA_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lang innledning"
SHORT_PREAMBLE_STR 			= "Kort innledning"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spania"
FRANCE_STR 				= "Frankrike"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Repeteringsgrense (i sek.) for roaming"
LEISURE_POWER_SAVE_STR			= "Stromsparing ved uvirksomhet"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Blinkintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.001d] ; Swedish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Natverkstyp"
LED_CONTROL_STR				= "LED-kontroll" 
POWER_SAVE_STR				= "Energisparlage"
WIFI_IBSS_STR				= "IBSS standard 11b Mode"
RATE_ADAPTIVE_STR			= "Anpassningsbar hastighet"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX radiomatning"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Offline matning (0: obegransat)"
FORCE_PRIORITY_STR			= "Tvingad prioritet"
HW_PARA_STR				= "Init fran HwParaFile"
THREE_WIRE_MODE_STR			= "Tretrads programmeringslage"
BOARD_TYPE_STR				= "Korttyp"
PROTECTION_MODE_STR			= "Skyddslage"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "Valj TPC-polaritet"
HIGH_POWER_STR				= "Hogkraftsmekanism"
INIT_GAIN_STR				= "Ursprungligt forstarkningslage"
CW_MAX_MIN_STR				= "Konkurrensfonster"
PSP_XLINK_STR				= "PSP XLink-lage"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Tradlost lage"
PREAMBLE_MODE_STR			= "Inledningslage"
FRAGTHRESH_STR				= "Fragmenteringstroskel"
RTSTHRESH_STR				= "RTS-troskel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Inaktivera"
ENABLE_STR 				= "Aktivera"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autoval"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lang inledning"
SHORT_PREAMBLE_STR 			= "Kort inledning"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankrike"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Grans for nytt roamingforsok (sek)"
LEISURE_POWER_SAVE_STR			= "Leisure energibesparning"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Fyrintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0006] ; Danish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Netvarkstype"
LED_CONTROL_STR				= "LED-kontrol" 
POWER_SAVE_STR				= "Stromstyrings-tilstand"
WIFI_IBSS_STR				= "IBSS standard 11b-tilstand"
RATE_ADAPTIVE_STR			= "Hastighed tilpasset"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX radiomaling"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX maks. offline-maling (0: ubegranset)"
FORCE_PRIORITY_STR			= "Forceret prioritet"
HW_PARA_STR				= "Init. fra HwParaFile"
THREE_WIRE_MODE_STR			= "Tre ledninger programmering-tilstand"
BOARD_TYPE_STR				= "Korttype"
PROTECTION_MODE_STR			= "Beskyttelse-tilstand"
TPC_STR					= "Overfor strom-kontrol"
TPC_POLARITY_STR			= "Valg TPC polaritet"
HIGH_POWER_STR				= "Hojeffekt-mekanisme"
INIT_GAIN_STR				= "Initiel forstarkning-tilstand"
CW_MAX_MIN_STR				= "Konflikt-vindue"
PSP_XLINK_STR				= "PSP XLink-tilstand"
CHANNEL_PLAN_STR			= "Kanal-plan"
WL_MODE_STR				= "Tradlos-tilstand"
PREAMBLE_MODE_STR			= "Start-tilstand"
FRAGTHRESH_STR				= "Fragmenteringstarskel"
RTSTHRESH_STR				= "RTS-tarskel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktiver"
ENABLE_STR 				= "Aktiver"
CAM_STR 				= "KAM"
MAX_PSP_STR 				= "MAKS._PSP"
FAST_PSP_STR 				= "Hurtig_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Auto-valg"
DOMAIN_FROM_EEPROM_STR 			= "DOMANE_FRA_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lang preamble"
SHORT_PREAMBLE_STR 			= "Kort preamble"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankrig"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Begransning for gentagne roam forsog (sek)"
LEISURE_POWER_SAVE_STR			= "Fritid - stromstyring"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Lys interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"

;;====================================================================================================================
[Strings.000b] ; Finnsih
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanava"
NETWORK_TYPE_STR 			= "Verkkotyyppi"
LED_CONTROL_STR				= "LED-hallinta" 
POWER_SAVE_STR				= "Virransaastotila"
WIFI_IBSS_STR				= "IBSS-oletus 11b-tila"
RATE_ADAPTIVE_STR			= "Nopeuteen mukautuva"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX-radiomittaus"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX-maksimi-offline-mittaus (0: rajoittamaton)"
FORCE_PRIORITY_STR			= "Pakotettu prioriteetti"
HW_PARA_STR				= "Alustus HwParaFilesta"
THREE_WIRE_MODE_STR			= "Kolmen langan ohjelmointitila"
BOARD_TYPE_STR				= "Levytyyppi"
PROTECTION_MODE_STR			= "Suojaustila"
TPC_STR					= "Virranhallinnan siirto"
TPC_POLARITY_STR			= "TPC-polariteetin valinta"
HIGH_POWER_STR				= "Korkeatehomekanismi"
INIT_GAIN_STR				= "Ensimmainen vahvistustila"
CW_MAX_MIN_STR				= "Vaiteikkuna"
PSP_XLINK_STR				= "PSP XLink -tila"
CHANNEL_PLAN_STR			= "Kanavasuunnitelma"
WL_MODE_STR				= "Langaton tila"
PREAMBLE_MODE_STR			= "Synkronointitila"
FRAGTHRESH_STR				= "Sirpaleisuuden kynnys"
RTSTHRESH_STR				= "RTS-kynnys"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Pois paalta"
ENABLE_STR 				= "Paalle"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktuuri"
AUTO_SELECT_STR 			= "Automaattinen valinta"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Autom."
LONG_PREAMBLE_STR 			= "Pitka tahdistuskuvio"
SHORT_PREAMBLE_STR 			= "Lyhyt tahdistuskuvio"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanja"
FRANCE_STR 				= "Ranska"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roamingin uudelleen yrittamisen rajoitus (sek.)"
LEISURE_POWER_SAVE_STR			= "Joutenolon virransaasto"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Paikkatietopakettien intervalli"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0019] ; Russian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Канал"
NETWORK_TYPE_STR 			= "Тип сети"
LED_CONTROL_STR				= "Индикатор" 
POWER_SAVE_STR				= "Режим энергосбережения"
WIFI_IBSS_STR				= "Режим IBSS Default 11b"
RATE_ADAPTIVE_STR			= "Адаптивная скорость"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: неограниченно)"
FORCE_PRIORITY_STR			= "Принудительный приоритет"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Режим Three Wire Programming Mode"
BOARD_TYPE_STR				= "Тип карты"
PROTECTION_MODE_STR			= "Защищенный режим"
TPC_STR					= "Управление мощностью передачи"
TPC_POLARITY_STR			= "Выбор полярности TPC"
HIGH_POWER_STR				= "Повышение мощности"
INIT_GAIN_STR				= "Первоначальное состояние усиления"
CW_MAX_MIN_STR				= "Окно соединения"
PSP_XLINK_STR				= "Режим PSP XLink"
CHANNEL_PLAN_STR			= "План каналов"
WL_MODE_STR				= "Режим беспроводной связи"
PREAMBLE_MODE_STR			= "Тип преамбулы"
FRAGTHRESH_STR				= "Порог фрагментации"
RTSTHRESH_STR				= "Порог RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Отключено"
ENABLE_STR 				= "Включено"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Прямое подключение"
INFRASTRUCTURE_STR 			= "Инфраструктура"
AUTO_SELECT_STR 			= "Автовыбор"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Авто"
LONG_PREAMBLE_STR 			= "Длинная преамбула"
SHORT_PREAMBLE_STR 			= "Короткая преамбула"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Испания"
FRANCE_STR 				= "Франция"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Израиль"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Лимит повтора роуминга (с)"
LEISURE_POWER_SAVE_STR			= "Энергосбережение при простое"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Интервал маяка"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0005] ; Czech
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanál"
NETWORK_TYPE_STR 			= "Typ sítě"
LED_CONTROL_STR				= "Indikátor LED" 
POWER_SAVE_STR				= "Režim úspory napájení"
WIFI_IBSS_STR				= "Výchozí režim IBSS 11b"
RATE_ADAPTIVE_STR			= "Přizpůsobivé na rychlost"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Měření rádia CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Max. měření offline CCX (0: neomezeno)"
FORCE_PRIORITY_STR			= "Vynucená priorita"
HW_PARA_STR				= "Inic z HwParaFile"
THREE_WIRE_MODE_STR			= "Režim programování Three Wire"
BOARD_TYPE_STR				= "Typ desky"
PROTECTION_MODE_STR			= "Režim ochrany"
TPC_STR					= "Řízení napájení přenosu"
TPC_POLARITY_STR			= "Výběr polarity TPC"
HIGH_POWER_STR				= "Mechanizmus s vysokým výkonem"
INIT_GAIN_STR				= "Počáteční stav zesílení"
CW_MAX_MIN_STR				= "Okno připojení"
PSP_XLINK_STR				= "Režim PSP XLink"
CHANNEL_PLAN_STR			= "Kanálový plán"
WL_MODE_STR				= "Bezdrátový režim"
PREAMBLE_MODE_STR			= "Režim preambule"
FRAGTHRESH_STR				= "Fragmentování prahové hodnoty"
RTSTHRESH_STR				= "Práh RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktivovat"
ENABLE_STR 				= "Aktivovat"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Rychlý_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktura"
AUTO_SELECT_STR 			= "Automatický výběr"
DOMAIN_FROM_EEPROM_STR 			= "DOMÉNA_Z_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Dlouhá preambule"
SHORT_PREAMBLE_STR 			= "Krátká preambule"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Španělsko"
FRANCE_STR 				= "Francie"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limit opakovaného pokusu o roaming(s.)"
LEISURE_POWER_SAVE_STR			= "Úsporný režim pro volný čas"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Interval blikání"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0015] ; Polsih
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR				= "SSID"
CHANNEL_STR				= "Kanał"
NETWORK_TYPE_STR			= "Rozdaj sieci"
LED_CONTROL_STR				= "Wskaźnik LED " 
POWER_SAVE_STR				= "Tryb oszczędzania energii"
WIFI_IBSS_STR				= "Tryb domyślny IBSS 11b "
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"

CCX_RM_STR				= "Pomiar sygnału radiowego CCX "
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Pomiar maks. CCX off-line (0: nieograniczony)"
FORCE_PRIORITY_STR			= "Wymuszone pierwszeństwo"
HW_PARA_STR				= "Inic z HwParaFile"
THREE_WIRE_MODE_STR			= "Trzyprzewodowy tryb programowania"
BOARD_TYPE_STR				= "Rodzaj płyty"
PROTECTION_MODE_STR			= "Tryb zabezpieczenia"
TPC_STR					= "Kontrola mocy nadawanej"
TPC_POLARITY_STR			= "Wybór biegunowości TPC "
HIGH_POWER_STR				= "Mechanizm wysokiej mocy"
INIT_GAIN_STR				= "Stan początkowego wzrostu"
CW_MAX_MIN_STR				= "Okno rywalizacji"
PSP_XLINK_STR				= "Tryb PSP XLink "
CHANNEL_PLAN_STR			= "Plan kanałów"
WL_MODE_STR				= "Tryb bezprzewodowy"
PREAMBLE_MODE_STR			= "Tryb preambuły"
FRAGTHRESH_STR				= "Próg fragmentacji"
RTSTHRESH_STR				= "Próg RTS "
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Wyłącz"
ENABLE_STR 				= "Włącz"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktura"
AUTO_SELECT_STR 			= "Automatyczne wybieranie"
DOMAIN_FROM_EEPROM_STR 			= "DOMENA_Z_EEPROM"
AUTO_STR 				= "Automatyczny"
LONG_PREAMBLE_STR 			= "Długa preambuła"
SHORT_PREAMBLE_STR 			= "Krótka preambuła "
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Hiszpania"
FRANCE_STR 				= "Francja"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Ograniczenie czasu wędrówki (sek.)"
LEISURE_POWER_SAVE_STR			= "Ograniczenie zużycia energii poza pracą"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Częstotliwość wysyłania ramek"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.001f] ; Turkish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Ağ Tipi"
LED_CONTROL_STR				= "LED Kontrolü" 
POWER_SAVE_STR				= "Güç Tasarruf Modu"
WIFI_IBSS_STR				= "IBSS Varsayılan 11b Modu"
RATE_ADAPTIVE_STR			= "Uyarlanır Oran"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radyo Ölçümü"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Maks Kapalı Hat Ölçümü (0: limitsiz)"
FORCE_PRIORITY_STR			= "Zorunlu Öncelik"
HW_PARA_STR				= "HwParaFile'dan Başlat"
THREE_WIRE_MODE_STR			= "Üç Kablo Programlama Modu"
BOARD_TYPE_STR				= "Kart Tipi"
PROTECTION_MODE_STR			= "Koruma Modu"
TPC_STR					= "İletim Gücü Denetimi"
TPC_POLARITY_STR			= "TPC Kutupsallık Seçimi"
HIGH_POWER_STR				= "Yüksek Güçlü Mekanizma"
INIT_GAIN_STR				= "İlk Edinim Durumu"
CW_MAX_MIN_STR				= "Tartışma Penceresi"
PSP_XLINK_STR				= "PSP XLink Modu"
CHANNEL_PLAN_STR			= "Kanal Planı"
WL_MODE_STR				= "Kablosuz Modu"
PREAMBLE_MODE_STR			= "Başlangıç Modu"
FRAGTHRESH_STR				= "Fragmentasyon Eşiği"
RTSTHRESH_STR				= "RTS Eşiği"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Devredışı Bırak"
ENABLE_STR 				= "Etkinleştir"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"

FAST_PSP_STR 				= "Hızlı_PSP"
AD_HOC_STR 				= "Geçici"
INFRASTRUCTURE_STR 			= "Altyapı"
AUTO_SELECT_STR 			= "Otomatik Seç"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Otomatik"
LONG_PREAMBLE_STR 			= "Uzun Başlangıç"
SHORT_PREAMBLE_STR 			= "Kısa Başlangıç"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "İspanya"
FRANCE_STR 				= "Fransa"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "İsrail"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Dolaşım Modu Yeniden Deneme Sınırı (sn)"
LEISURE_POWER_SAVE_STR			= "Boş Zaman Güç Tasarrufu"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "İşaret Aralığı"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.000e] ; Hungarian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Csatorna"
NETWORK_TYPE_STR 			= "Hálózat típusa"
LED_CONTROL_STR				= "LED-vezérlés" 
POWER_SAVE_STR				= "Energiatakarékos mód"
WIFI_IBSS_STR				= "IBSS alapértelmezett 11b mód"
RATE_ADAPTIVE_STR			= "Adaptív sebességválasztás"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX rádiómérés"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line mérés (0: korlátlan)"
FORCE_PRIORITY_STR			= "Erőltetett elsőbbség"
HW_PARA_STR				= "Inicializálás innen: HwParaFile"
THREE_WIRE_MODE_STR			= "Háromvezetékes programozási mód"
BOARD_TYPE_STR				= "Paneltípus"
PROTECTION_MODE_STR			= "Védett mód"
TPC_STR					= "Sugárzási teljesítményvezérlés"

TPC_POLARITY_STR			= "TPC polaritás választás"
HIGH_POWER_STR				= "Nagyteljesítményű mechanizmus"
INIT_GAIN_STR				= "Kezdeti erősítési állapot"
CW_MAX_MIN_STR				= "Vetélkedési ablak"
PSP_XLINK_STR				= "PSP XLink mód"
CHANNEL_PLAN_STR			= "Csatornaterv"

WL_MODE_STR				= "Vezeték nélküli mód"
PREAMBLE_MODE_STR			= "Előtag mód"
FRAGTHRESH_STR				= "Tördelési küszöb"
RTSTHRESH_STR				= "RTS küszöb"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Letiltás"
ENABLE_STR 				= "Engedélyezés"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktúra"
AUTO_SELECT_STR 			= "Automata választás"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Automata"
LONG_PREAMBLE_STR 			= "Hosszú előtag"
SHORT_PREAMBLE_STR 			= "Rövid előtag"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanyolország"
FRANCE_STR 				= "Franciaország"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Barangolás újraindításának időkorlátja (mp)"
LEISURE_POWER_SAVE_STR			= "Energiatakarékos mód szórakoztató eszközökhöz"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Jelzés időköze"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0008] ; Greek
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Κανάλι"
NETWORK_TYPE_STR 			= "Τύπος Δικτύου"
LED_CONTROL_STR				= "Ενδείξεις λυχνιών LED" 
POWER_SAVE_STR				= "Λειτουργία εξοικονόμησης ενέργειας"
WIFI_IBSS_STR				= "IBSS Προεπιλεγμένη λειτουργία 11b"
RATE_ADAPTIVE_STR			= "Προσαρμόσιμη ταχύτητα"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Ραδιομέτρηση CCX"

CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Μέγιστη μέτρηση εκτός σύνδεσης CCX (0: απεριόριστο)"
FORCE_PRIORITY_STR			= "Εξαναγκασμένη προτεραιότητα"
HW_PARA_STR				= "Αρχικοποίηση από HwParaFile"
THREE_WIRE_MODE_STR			= "Λειτουργία προγραμματισμού τριών καλωδίων"
BOARD_TYPE_STR				= "Τύπος κάρτας"
PROTECTION_MODE_STR			= "Λειτουργία προστασίας"
TPC_STR					= "Έλεγχος μετάδοσης ισχύος"
TPC_POLARITY_STR			= "Επιλογή πολικότητας TPC"
HIGH_POWER_STR				= "Μηχανισμός υψηλής ισχύος"
INIT_GAIN_STR				= "Κατάσταση αρχικού οφέλους"
CW_MAX_MIN_STR				= "Παράθυρο διεκδίκησης"
PSP_XLINK_STR				= "Λειτουργία PSP XLink"
CHANNEL_PLAN_STR			= "Σχέδιο καναλιού"
WL_MODE_STR				= "Λειτουργία ασύρματου"
PREAMBLE_MODE_STR			= "Λειτουργία μπλοκ εισαγωγής"
FRAGTHRESH_STR				= "Κατώφλι τμήματος"
RTSTHRESH_STR				= "Κατώφλι RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Απενεργοποίηση"
ENABLE_STR 				= "Ενεργοποίηση"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Λειτουργία Ad-hoc"
INFRASTRUCTURE_STR 			= "Υποδομή"
AUTO_SELECT_STR 			= "Αυτόματη επιλογή"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Αυτόματο"
LONG_PREAMBLE_STR 			= "Μεγάλο μπλοκ εισαγωγής"
SHORT_PREAMBLE_STR 			= "Μικρό μπλοκ εισαγωγής"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Ισπανία"
FRANCE_STR 				= "Γαλλία"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Ισραήλ"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Όριο επαναλήψεων προσπάθειας περιαγωγής (δευτ.)"
LEISURE_POWER_SAVE_STR			= "Εξοικονόμηση ενέργειας σε κατάσταση αδράνειας"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Διάστημα προειδοποιητικού σήματος"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.001b] ; Slovak
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanál"
NETWORK_TYPE_STR 			= "Typ siete"
LED_CONTROL_STR				= "LED indikátor" 
POWER_SAVE_STR				= "Režim úspory energie"
WIFI_IBSS_STR				= "Predvolený 11b režim IBSS"
RATE_ADAPTIVE_STR			= "Prispôsobiteľný rýchlosti"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Rádiové meranie pre CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Off line meranie pre CCX Max (0: bez obmedzenia)"
FORCE_PRIORITY_STR			= "Vynútená priorita"
HW_PARA_STR				= "Inicializácia zo súboru HwParaFile"
THREE_WIRE_MODE_STR			= "Trojvodičový režim programovania"
BOARD_TYPE_STR				= "Typ dosky"
PROTECTION_MODE_STR			= "Režim ochrany"
TPC_STR					= "Ovládanie vysielacieho výkonu"
TPC_POLARITY_STR			= "Voľba TPC polarity"
HIGH_POWER_STR				= "Vysoko výkonný mechanizmus"
INIT_GAIN_STR				= "Počiatočný stav získavania"
CW_MAX_MIN_STR				= "Okno pripojenia"
PSP_XLINK_STR				= "Režim linky PSP XLink"
CHANNEL_PLAN_STR			= "Prehľad kanálov"
WL_MODE_STR				= "Bezdrôtový režim"
PREAMBLE_MODE_STR			= "Úvodný režim"
FRAGTHRESH_STR				= "Prahová hodnota pre fragmentáciu"
RTSTHRESH_STR				= "Prahová hodnota pre RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktivovať"
ENABLE_STR 				= "Aktivovať"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Rýchly_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infraštruktúra"
AUTO_SELECT_STR 			= "Automatická voľba"
DOMAIN_FROM_EEPROM_STR 			= "DOMÉNA_Z_EEPROM"
AUTO_STR 				= "Automaticky"
LONG_PREAMBLE_STR 			= "Dlhý úvod"
SHORT_PREAMBLE_STR 			= "Krátky úvod"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Španielsko"
FRANCE_STR 				= "Francúzsko"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= " Limit(sek) opakovania roamingu "
LEISURE_POWER_SAVE_STR			= " Oddychový úsporný režim "
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= " Interval majáka "


SSID_STR				= "SSID"
CHANNEL_STR				= "แชนเนล"
NETWORK_TYPE_STR			= "ชนิดเน็ตเวิร์ก"
LED_CONTROL_STR				= "LED ควบคุม" 
POWER_SAVE_STR				= "โหมดประหยัดพลังงาน"
WIFI_IBSS_STR				= "โหมด IBSS เริ่มต้น 11b "
RATE_ADAPTIVE_STR			= "อัตราอะแดปทีฟ"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "การวัดวิทยุ CCX "
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "การวัด CCX ออฟไลน์สูงสุด (0: ไม่จำกัด)"
FORCE_PRIORITY_STR			= "ลำดับความสำคัญที่ถูกบังคับ"
HW_PARA_STR				= "ตั้งค่าเริ่มต้นจาก HwParaFile"
THREE_WIRE_MODE_STR			= "โหมดการโปรแกรม 3 สาย"
BOARD_TYPE_STR				= "ชนิดบอร์ด"
PROTECTION_MODE_STR			= "โหมดการป้องกัน"
TPC_STR					= "ควบคุมพลังงานการส่ง"
TPC_POLARITY_STR			= "เลือกขั้ว TPC "
HIGH_POWER_STR				= "กลไกพลังงานสูง"
INIT_GAIN_STR				= "สถานะเกนเริ่มแรก"
CW_MAX_MIN_STR				= "หน้าต่างการยืนยัน"
PSP_XLINK_STR				= "โหมด PSP XLink "
CHANNEL_PLAN_STR			= "แผนแชนเนล"
WL_MODE_STR				= "โหมดไร้สาย"
PREAMBLE_MODE_STR			= "โหมดส่วนเริ่มต้น"
FRAGTHRESH_STR				= "ขอบเขตชิ้นส่วน"
RTSTHRESH_STR				= "ขอบเขต RTS "
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "ปิดทำงาน"
ENABLE_STR 				= "เปิดทำงาน"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "โครงสร้างพื้นฐาน"
AUTO_SELECT_STR 			= "เลือกอัตโนมัติ"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "อัตโนมัติ"
LONG_PREAMBLE_STR 			= "ส่วนเริ่มต้นยาว"
SHORT_PREAMBLE_STR 			= "ส่วนเริ่มต้นสั้น"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "สเปน"
FRANCE_STR 				= "ฝรั่งเศส"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "อิสราเอล"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "ขีดจำกัดการลองโรมใหม่ (วินาที)"
LEISURE_POWER_SAVE_STR			= "การประหยัดพลังงานขณะที่ว่าง"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "ช่วงไฟสัญญาณ"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0001] ; Arabic (Saudi Arabia)
Realtek 				= "شركة Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR				= "معرف SSID"
CHANNEL_STR				= "القناة"
NETWORK_TYPE_STR			= "نوع الشبكة"
LED_CONTROL_STR				= "التحكم في مؤشر بيان الحالة" 
POWER_SAVE_STR				= "وضع توفير الطاقة"
WIFI_IBSS_STR				= "وضع 11b الافتراضي لـ IBSS"
RATE_ADAPTIVE_STR			= "مهايئ المعدل"
QOS_STR					= "جودة الخدمة"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "القياس اللاسلكي لـ CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "الحد الأقصى لقياس CCX عند عدم الاتصال (0: غير محدود)"
FORCE_PRIORITY_STR			= "الأولوية الإجبارية"
HW_PARA_STR				= "بدء التهيئة من ملف HwparaFile"
THREE_WIRE_MODE_STR			= "وضع البرمجة ثلاثي الأسلاك"
BOARD_TYPE_STR				= "نوع اللوحة"
PROTECTION_MODE_STR			= "وضع الحماية"
TPC_STR					= "نقل التحكم في الطاقة"
TPC_POLARITY_STR			= "تحديد قطبية TPC"
HIGH_POWER_STR				= "آلية الطاقة المرتفعة"
INIT_GAIN_STR				= "حالة الكسب الأولية"
CW_MAX_MIN_STR				= "نافذة التعارض"
PSP_XLINK_STR				= "وضع PSP XLink"
CHANNEL_PLAN_STR			= "خطة القناة"
WL_MODE_STR				= "الوضع اللاسلكي"
PREAMBLE_MODE_STR			= "وضع الإشارة الابتدائية"
FRAGTHRESH_STR				= "حد التجزئة"
RTSTHRESH_STR				= "حد RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "تعطيل"
ENABLE_STR 				= "تمكين"
CAM_STR 				= "الكامة"
MAX_PSP_STR 				= "الحد الأقصى لـ PSP"
FAST_PSP_STR 				= "PSP سريع"
AD_HOC_STR 				= "عشوائي"
INFRASTRUCTURE_STR 			= "البنية الأساسية"
AUTO_SELECT_STR 			= "تحديد تلقائي"
DOMAIN_FROM_EEPROM_STR 			= "المجال من EEPROM"
AUTO_STR 				= "تلقائي"
LONG_PREAMBLE_STR 			= "إشارة ابتدائية طويلة"
SHORT_PREAMBLE_STR 			= "إشارة ابتدائية قصيرة"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "اللجنة الفيدرالية للاتصالات"
IC_STR 					= "دائرة متكاملة"
ETSI_STR 				= "معهد معايير الاتصالات السلكية واللاسلكية"
SPAIN_STR 				= "إسبانيا"
FRANCE_STR 				= "فرنسا"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "إسرائيل"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "حد تكرار التجوال (بالثواني)"
LEISURE_POWER_SAVE_STR			= "توفير الطاقة عند عدم الاستخدام"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "فاصل Beacon الزمني"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.000d] ; Hebrew
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR				= "SSID"
CHANNEL_STR				= "ערוץ"
NETWORK_TYPE_STR			= "סוג רשת"
LED_CONTROL_STR				= "בקרת נוריות" 
POWER_SAVE_STR				= "מצב חיסכון בצריכת חשמל"
WIFI_IBSS_STR				= "מצב ברירת מחדל 11b ל-IBSS"
RATE_ADAPTIVE_STR			= "קצב מותאם"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "ערך שידור CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "ערך CCX מרבי במצב לא מקוון (0:  ללא הגבלה)"
FORCE_PRIORITY_STR			= "עדיפות מאולצת"
HW_PARA_STR				= "אתחל מקובץ HwParaFile"
THREE_WIRE_MODE_STR			= "מצב תכנות Three Wire"
BOARD_TYPE_STR				= "סוג לוח"
PROTECTION_MODE_STR			= "מצב הגנה"
TPC_STR					= "בקרת הספק שידור"
TPC_POLARITY_STR			= "בחירת קוטביות TPC"
HIGH_POWER_STR				= "מנגנון הספק גבוה"
INIT_GAIN_STR				= "מצב הגבר התחלתי"
CW_MAX_MIN_STR				= "חלון Contention"
PSP_XLINK_STR				= "מצב PSP XLink"
CHANNEL_PLAN_STR			= "תכנון ערוצים"
WL_MODE_STR				= "מצב אלחוטי"
PREAMBLE_MODE_STR			= "מצב מקדים"
FRAGTHRESH_STR				= "סף פיצול"
RTSTHRESH_STR				= "סף RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "חסום"
ENABLE_STR 				= "אפשר"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "אד הוק"
INFRASTRUCTURE_STR 			= "תשתית"
AUTO_SELECT_STR 			= "בחירה אוטומטית"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "אוטומטי"
LONG_PREAMBLE_STR 			= "מקדים ארוך"
SHORT_PREAMBLE_STR 			= "מקים קצר"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "ספרד"
FRANCE_STR 				= "צרפת"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "ישראל"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "הגבלת ניסיון חוזר לנדידה (שניות)"
LEISURE_POWER_SAVE_STR			= "מצב חיסכון בחשמל בזמן המתנה"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "מרווח זמן למשואה"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
;;====================================================================================================================
[Strings.0416] ; Portuguese (Brazil)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"

SSID_STR				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR			= "Tipo de Rede"
LED_CONTROL_STR				= "Controle de LED" 
POWER_SAVE_STR				= "Modo de Economia de Energia"
WIFI_IBSS_STR				= "Modo IBSS Default 11b"
RATE_ADAPTIVE_STR			= "Adaptativo à Taxa"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Medida de Rádio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medida offline máx. CCX (0: ilimitada)"
FORCE_PRIORITY_STR			= "Prioridade Forçada"
HW_PARA_STR				= "Inicialização de HwParaFile"
THREE_WIRE_MODE_STR			= "Modo de programação de três fios"
BOARD_TYPE_STR				= "Tipo de placa"
PROTECTION_MODE_STR			= "Modo de Proteção"
TPC_STR					= "Controle de Potência de Transmissão"
TPC_POLARITY_STR			= "Seleção de Polaridade TPC"
HIGH_POWER_STR				= "Mecanismo de Alta Potência"
INIT_GAIN_STR				= "Estado de Ganho Inicial"
CW_MAX_MIN_STR				= "Janela de Contenção"
PSP_XLINK_STR				= "Modo PSP XLink"
CHANNEL_PLAN_STR			= "Plano de Canal"

WL_MODE_STR				= "Modo Wireless"
PREAMBLE_MODE_STR			= "Modo de Preâmbulo"
FRAGTHRESH_STR				= "Limite de Fragmentação"
RTSTHRESH_STR				= "Limite RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Desabilitar"
ENABLE_STR 				= "Habilitar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "PSP MÁX"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infra-estrutura"
AUTO_SELECT_STR 			= "Seleção automática"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Automático"
LONG_PREAMBLE_STR 			= "Preâmbulo longo"
SHORT_PREAMBLE_STR 			= "Preâmbulo curto"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "CI"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanha"
FRANCE_STR 				= "França"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite de Tentativas de Roam (seg)"
LEISURE_POWER_SAVE_STR			= "Economia de Energia de Descanso"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Intervalo de Sinal"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTL8192CeT.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc		="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc		="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc		="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc 		="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc		="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc	="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc	="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
RTL8192de0.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC0"
RTL8192de1.DeviceDesc		="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName	="Realtek RTL8192DE Wireless LAN 802.11N PCI-E NIC MAC1"
RTL8723ae.DeviceDesc		="Realtek RTL8723AE Wireless LAN 802.11n PCI-E NIC"
LNV8723ae.DeviceDesc		="1x1 11b/g/n Wireless LAN M.2 Adapter"
RTL8188e.DeviceDesc		="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
RTL8188e.DeviceDesc.DispName	="Realtek RTL8188E Wireless LAN 802.11n PCI-E NIC"
HP8188e.DeviceDesc		="Realtek RTL8188EE 802.11bgn Wi-Fi Adapter"
RTL8812e.DeviceDesc		="Realtek RTL8812E Wireless LAN 802.11n PCI-E NIC"
RTL8821e.DeviceDesc		="Realtek RTL8821E Wireless LAN 802.11n PCI-E NIC"
